Firmware upgrade

1. Install program for programming new firmware - English UP-2.44.
2. Easy setting this program - use INI file UP.INI and copy this file into install directory of program UP-2.24
3. Picture of setting this programm
4. Schematic of the special programming cable
5. Driver USB for PRESTO programmer
6. Manual of use interface Presto in English language

Firmware version:

V3.0 start basic firmware (12.3.2006)

V3.1 repair feature of reading buttons (12.12.2006)

V3.2 - dtto - for another customer

V3.3 new feature of relay - switch 2 impulses for automatic gates (24.10.2007)

V3.4 new feature of tone detection - enable setting signalling tone parameters (4.1.2008)

V3.5 - dtto - for another customer

V3.6 new inicialization control watchdog 12.3.2008) last version for version board to the V1.9

V 3.7 - dtto - for another customer

V3.8 - dtto - for another customer

V4.0 - Version with possibilities connection SlimKeyBoard (15.12.2009) only for version board from V2.0

V4.1 - dtto - for another customer

V4.2 - dtto - for another customer