#!version:1.0.0.1

##File header "#!version:1.0.0.1" can not be edited or deleted.##

#######################################################################################
##                                   Account1 Settings                               ##                                       
#######################################################################################

#Enable or disable the account 1; 0-Disabled (default), 1-Enabled;
account.1.enable = %BWLINE-BINARY-1%

#Configure the label displayed on the LCD screen for account 1.
account.1.label = %BWEXTENSION-1%

#Configure the display name of account 1.
account.1.display_name = %BWCLID-1%

#Configure the username and password for register authentication.
account.1.auth_name = %BWAUTHUSER-1%
account.1.password = %BWAUTHPASSWORD-1%

#Configure the register user name.
account.1.user_name = %BWLINEPORT-1%



#Enable or disable to use the outbound proxy server; 0-Disabled (default), 1-Enabled; 
account.1.outbound_proxy_enable = 1

#Specify the IP address or domain name of the outbound proxy server.
account.1.outbound_host = %SBC_ADDRESS%

#Specify the server port, the default value is 5060.
account.1.outbound_port = %SBC_PORT%

#Configure the transport type; 0-UDP (default), 1-TCP, 2-TLS, 3-DNS SRV;
account.1.transport = %TRANSPORT_TYPE%

 
voice_mail.number.1 = %BWVOICE-PORTAL-NUMBER-1% 
account.1.anonymous_call_mode =
account.1.reject_anonymous_call_mode =

#Enable or disable the anonymous call feature; 0-Disabled (default), 1-Enabled;
account.1.anonymous_call = 


#Enable or disable the reject anonymous call feature; 0-Disabled (default), 1-Enabled;
account.1.reject_anonymous_call = %REJECT_ANONYMOUS_CALL_BINARY%


#Configure the SIP port for account 1, the default value is 5060. 
account.1.sip_listen_port = 

#Configure the register expiry time (in seconds), the default value is 3600.
account.1.expires = 

#Enable or disable the 100 reliable retransmission; 0-Disabled, 1-Enabled (default);
account.1.100rel_enable =


#Enable or disable the phone to subscribe the register status; 0-Disabled (default), 1-Enabled;
account.1.subscribe_register =

#Enable or disable the phone to subscribe the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.1.subscribe_mwi = 

#Configure MWI subscribe expiry time (in seconds). It ranges from 0 to 84600, the default value is 3600.
account.1.subscribe_mwi_expires = 

#Configure the type of SIP header to carry the caller ID; 0-FROM (default), 1-PAI;
account.1.cid_source = 
 
#Enable or disable the session timer; 0-Disabled (default), 1-Enabled;  
account.1.session_timer.enable =       

#Configure the refresh session timer interval (in seconds). It ranges from 1 to 9999.
account.1.session_timer.expires =           

#Configure the session timer refresher; 0-Uac (default), 1-Uas;
account.1.session_timer.refresher = 

#Enable or disable the "user=phone"; 0-Disabled (default), 1-Enabled;
account.1.enable_user_equal_phone = 

#Configure the way of encrypting the message; 0-Disabled (default), 1-Forced, 2-Negotiated;
account.1.srtp_encryption = 

#Configure the RTP packet time. The valid values are 0 (Disabled), 10, 20 (default), 30, 40, 50, 60.
account.1.ptime =  

#Enable or disable the phone to subscribe to the voicemail through the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.1.subscribe_mwi_to_vm = 

#Enable or disable the phone to send the MAC address in the Register message; 0-Disabled (default), 1-Enabled;    
account.1.register_mac =

#Enable or disable the phone to send the line number in the Register message; 0-Disabled, 1-Enabled (default);   
account.1.register_line = 

#Configure the interval (in seconds) the phone retries to register when account 1 fails to register. It ranges from 0 to 1800, the default value is 30.
account.1.reg_fail_retry_interval = 

#Configure the DTMF type; 0-INBAND, 1-RFC2833 (default), 2-SIP INFO, 3-AUTO+SIP INFO;
account.1.dtmf.type =

#Configure the RFC2833 payload. It ranges from 96 to 225, the default value is 101.
account.1.dtmf.dtmf_payload = 

#Configure the DTMF info type when using the SIP INFO; 0-Disabled, 1-DTMF-Relay (default), 2-DTMF, 3-Telephone-Event;
account.1.dtmf.info_type = 

account.1.auto_dial_num = 
account.1.auto_dial_enable = 

account.1.cid_source_privacy = 
account.1.cid_source_ppi = 
account.1.cp_source = 

voice_mail.number.1 = 

account.1.shared_line = 
#######################################################################################
##                          Failback                                                 ##       
#######################################################################################
account.1.naptr_build = 
account.1.fallback.redundancy_type = 
account.1.fallback.timeout = 
account.1.sip_server.1.address =
account.1.sip_server.1.port = 
account.1.sip_server.1.expires = 
account.1.sip_server.1.retry_counts = 
account.1.sip_server.1.failback_mode = 
account.1.sip_server.1.failback_timeout = 
account.1.sip_server.1.register_on_enable = 

account.1.sip_server.2.address =
account.1.sip_server.2.port = 
account.1.sip_server.2.expires = 
account.1.sip_server.2.retry_counts = 
account.1.sip_server.2.failback_mode = 
account.1.sip_server.2.failback_timeout = 
account.1.sip_server.2.register_on_enable = 

account.1.dns_cache_type = 
account.1.dns_cache_a.1.name =
account.1.dns_cache_a.1.ip =
account.1.dns_cache_a.1.ttl = 
account.1.dns_cache_srv.1.name =
account.1.dns_cache_srv.1.port = 
account.1.dns_cache_srv.1.priority = 
account.1.dns_cache_srv.1.target =
account.1.dns_cache_srv.1.weight = 
account.1.dns_cache_srv.1.ttl = 
account.1.dns_cache_naptr.1.name =
account.1.dns_cache_naptr.1.flags =
account.1.dns_cache_naptr.1.order = 
account.1.dns_cache_naptr.1.preference = 
account.1.dns_cache_naptr.1.replace =
account.1.dns_cache_naptr.1.service =
account.1.dns_cache_naptr.1.ttl = 


account.1.dns_cache_a.2.name =
account.1.dns_cache_a.2.ip =
account.1.dns_cache_a.2.ttl = 
account.1.dns_cache_srv.2.name =
account.1.dns_cache_srv.2.port = 
account.1.dns_cache_srv.2.priority = 
account.1.dns_cache_srv.2.target =
account.1.dns_cache_srv.2.weight = 
account.1.dns_cache_srv.2.ttl = 
account.1.dns_cache_naptr.2.name =
account.1.dns_cache_naptr.2.flags =
account.1.dns_cache_naptr.2.order = 
account.1.dns_cache_naptr.2.preference = 
account.1.dns_cache_naptr.2.replace =
account.1.dns_cache_naptr.2.service =
account.1.dns_cache_naptr.2.ttl = 

account.1.static_cache_pri = 






#######################################################################################
##                                   NAT Settings                                    ##
#######################################################################################

#Enable or disable the NAT traversal; 0-Disabled (default), 1-STUN;
account.1.nat.nat_traversal =

#Configure the STUN server address.
account.1.nat.stun_server = 

#Configure the STUN server port, the default value is 3478.
account.1.nat.stun_port = 

#Enable or disable the NAT keep-alive; 0-Disabled, 1-Enabled (default);
account.1.nat.udp_update_enable = 

#Specify the keep-alive interval (in seconds), the default value is 30.
account.1.nat.udp_update_time = 

#Enable or disable the NAT Rport; 0-Disabled (default), 1-Enabled;
account.1.nat.rport = 

#Configure the session timer (in seconds), the default values of T1, T2, T3 are 0.5, 4, 5.
account.1.advanced.timer_t1 = 
account.1.advanced.timer_t2 = 
account.1.advanced.timer_t4 = 

account.1.codec.1.enable = 
account.1.codec.1.payload_type = 
account.1.codec.1.priority = 
account.1.codec.1.rtpmap = 

account.1.codec.2.enable = 
account.1.codec.2.payload_type = 
account.1.codec.2.priority =  
account.1.codec.2.rtpmap = 

account.1.codec.3.enable = 
account.1.codec.3.payload_type = 
account.1.codec.3.priority =
account.1.codec.3.rtpmap = 

account.1.codec.4.enable = 
account.1.codec.4.payload_type = 
account.1.codec.4.priority = 
account.1.codec.4.rtpmap = 

account.1.codec.5.enable = 
account.1.codec.5.payload_type = 
account.1.codec.5.priority = 
account.1.codec.5.rtpmap = 

account.1.codec.6.enable = 
account.1.codec.6.payload_type = 
account.1.codec.6.priority = 
account.1.codec.6.rtpmap = 

account.1.codec.7.enable = 
account.1.codec.7.payload_type = 
account.1.codec.7.priority = 
account.1.codec.7.rtpmap = 

account.1.codec.8.enable =  
account.1.codec.8.payload_type = 
account.1.codec.8.priority = 
account.1.codec.8.rtpmap = 

account.1.codec.9.enable = 
account.1.codec.9.payload_type = 
account.1.codec.9.priority = 
account.1.codec.9.rtpmap = 

#######################################################################################
##         	                   Call Forward                                          ##               
#######################################################################################
#Enable or disable the always forward, 0-Disabled(default), 1-Enabled;
account.1.always_fwd.enable = 

#Configure the target phonenumber that the phone will forward the call to;
account.1.always_fwd.target = 




#Enable or disable the busy forward, 0-Disabled(default), 1-Enabled;
account.1.busy_fwd.enable =         
account.1.busy_fwd.target = 




#Enable or disable the no answer forward, 0-Disabled(default), 1-Enabled; 
#Configure the waiting ring times before forwarding, ranges from 0 to 20 (by default);
account.1.timeout_fwd.enable = 
account.1.timeout_fwd.target =
account.1.timeout_fwd.timeout =  



#######################################################################################
##                          DND                                                      ##                                       
#######################################################################################

#Enable or disable the DND feautre for account2; 0-Disabled (default), 1-Enabled;
account.1.dnd.enable = 



#######################################################################################
##                           Register Advanced                                       ##       
#######################################################################################
account.1.sip_server_type = 
account.1.unregister_on_reboot = 
account.1.sip_trust_ctrl = 
account.1.proxy_require = 
account.1.srv_ttl_timer_enable = 

#######################################################################################
##                                   Network Conference                              ##                                       
#######################################################################################
account.1.conf_type = 
account.1.conf_uri = 

#######################################################################################
##                                   Account2 Settings                               ##                                       
#######################################################################################

#Enable or disable the account 1; 0-Disabled (default), 1-Enabled;
account.2.enable = %BWLINE-BINARY-2%

#Configure the label displayed on the LCD screen for account 1.
account.2.label = %BWEXTENSION-2%

#Configure the display name of account 1.
account.2.display_name = %BWCLID-2%

#Configure the username and password for register authentication.
account.2.auth_name = %BWAUTHUSER-2%
account.2.password = %BWAUTHPASSWORD-2%

#Configure the register user name.
account.2.user_name = %BWLINEPORT-2%



#Enable or disable to use the outbound proxy server; 0-Disabled (default), 1-Enabled; 
account.2.outbound_proxy_enable = 1

#Specify the IP address or domain name of the outbound proxy server.
account.2.outbound_host = %SBC_ADDRESS%

#Specify the server port, the default value is 5060.
account.2.outbound_port = %SBC_PORT%

#Configure the transport type; 0-UDP (default), 1-TCP, 2-TLS, 3-DNS SRV;
account.2.transport = %TRANSPORT_TYPE%


voice_mail.number.2 = %BWVOICE-PORTAL-NUMBER-2% 
account.2.anonymous_call_mode =
account.2.reject_anonymous_call_mode =

#Enable or disable the anonymous call feature; 0-Disabled (default), 1-Enabled;
account.2.anonymous_call = 

#Configure the on code and off code of the anonymous call feature.
account.2.send_anonymous_code =
account.2.anonymous_call_oncode = 
account.2.anonymous_call_offcode = 

#Enable or disable the reject anonymous call feature; 0-Disabled (default), 1-Enabled;
account.2.reject_anonymous_call = %REJECT_ANONYMOUS_CALL_BINARY%

#Configure the on code and off code of the reject anonymous call feature.
account.2.send_anonymous_rejection_code =
account.2.anonymous_reject_oncode = 
account.2.anonymous_reject_offcode = 

#Configure the SIP port for account 1, the default value is 5060. 
account.2.sip_listen_port = 

#Configure the register expiry time (in seconds), the default value is 3600.
account.2.expires = 

#Enable or disable the 100 reliable retransmission; 0-Disabled, 1-Enabled (default);
account.2.100rel_enable =


#Enable or disable the phone to subscribe the register status; 0-Disabled (default), 1-Enabled;
account.2.subscribe_register =

#Enable or disable the phone to subscribe the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.2.subscribe_mwi = 

#Configure MWI subscribe expiry time (in seconds). It ranges from 0 to 84600, the default value is 3600.
account.2.subscribe_mwi_expires = 

#Configure the type of SIP header to carry the caller ID; 0-FROM (default), 1-PAI;
account.2.cid_source = 
 
#Enable or disable the session timer; 0-Disabled (default), 1-Enabled;  
account.2.session_timer.enable =       

#Configure the refresh session timer interval (in seconds). It ranges from 1 to 9999.
account.2.session_timer.expires =           

#Configure the session timer refresher; 0-Uac (default), 1-Uas;
account.2.session_timer.refresher = 

#Enable or disable the "user=phone"; 0-Disabled (default), 1-Enabled;
account.2.enable_user_equal_phone = 

#Configure the way of encrypting the message; 0-Disabled (default), 1-Forced, 2-Negotiated;
account.2.srtp_encryption = 

#Configure the RTP packet time. The valid values are 0 (Disabled), 10, 20 (default), 30, 40, 50, 60.
account.2.ptime =  

#Enable or disable the phone to subscribe to the voicemail through the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.2.subscribe_mwi_to_vm = 

#Enable or disable the phone to send the MAC address in the Register message; 0-Disabled (default), 1-Enabled;    
account.2.register_mac =

#Enable or disable the phone to send the line number in the Register message; 0-Disabled, 1-Enabled (default);   
account.2.register_line = 

#Configure the interval (in seconds) the phone retries to register when account 1 fails to register. It ranges from 0 to 1800, the default value is 30.
account.2.reg_fail_retry_interval = 

#Configure the DTMF type; 0-INBAND, 1-RFC2833 (default), 2-SIP INFO, 3-AUTO+SIP INFO;
account.2.dtmf.type =

#Configure the RFC2833 payload. It ranges from 96 to 225, the default value is 101.
account.2.dtmf.dtmf_payload = 

#Configure the DTMF info type when using the SIP INFO; 0-Disabled, 1-DTMF-Relay (default), 2-DTMF, 3-Telephone-Event;
account.2.dtmf.info_type = 

account.2.auto_dial_num = 
account.2.auto_dial_enable = 

account.2.cid_source_privacy = 
account.2.cid_source_ppi = 
account.2.cp_source = 

voice_mail.number.2 = 

account.2.shared_line = 
#######################################################################################
##                          Failback                                                 ##       
#######################################################################################
account.2.naptr_build = 
account.2.fallback.redundancy_type = 
account.2.fallback.timeout = 
account.2.sip_server.1.address =
account.2.sip_server.1.port = 
account.2.sip_server.1.expires = 
account.2.sip_server.1.retry_counts = 
account.2.sip_server.1.failback_mode = 
account.2.sip_server.1.failback_timeout = 
account.2.sip_server.1.register_on_enable = 

account.2.sip_server.2.address =
account.2.sip_server.2.port = 
account.2.sip_server.2.expires = 
account.2.sip_server.2.retry_counts = 
account.2.sip_server.2.failback_mode = 
account.2.sip_server.2.failback_timeout = 
account.2.sip_server.2.register_on_enable = 

account.2.dns_cache_type = 
account.2.dns_cache_a.1.name =
account.2.dns_cache_a.1.ip =
account.2.dns_cache_a.1.ttl = 
account.2.dns_cache_srv.1.name =
account.2.dns_cache_srv.1.port = 
account.2.dns_cache_srv.1.priority = 
account.2.dns_cache_srv.1.target =
account.2.dns_cache_srv.1.weight = 
account.2.dns_cache_srv.1.ttl = 
account.2.dns_cache_naptr.1.name =
account.2.dns_cache_naptr.1.flags =
account.2.dns_cache_naptr.1.order = 
account.2.dns_cache_naptr.1.preference = 
account.2.dns_cache_naptr.1.replace =
account.2.dns_cache_naptr.1.service =
account.2.dns_cache_naptr.1.ttl = 


account.2.dns_cache_a.2.name =
account.2.dns_cache_a.2.ip =
account.2.dns_cache_a.2.ttl = 
account.2.dns_cache_srv.2.name =
account.2.dns_cache_srv.2.port = 
account.2.dns_cache_srv.2.priority = 
account.2.dns_cache_srv.2.target =
account.2.dns_cache_srv.2.weight = 
account.2.dns_cache_srv.2.ttl = 
account.2.dns_cache_naptr.2.name =
account.2.dns_cache_naptr.2.flags =
account.2.dns_cache_naptr.2.order = 
account.2.dns_cache_naptr.2.preference = 
account.2.dns_cache_naptr.2.replace =
account.2.dns_cache_naptr.2.service =
account.2.dns_cache_naptr.2.ttl = 

account.2.static_cache_pri = 






#######################################################################################
##                                   NAT Settings                                    ##
#######################################################################################

#Enable or disable the NAT traversal; 0-Disabled (default), 1-STUN;
account.2.nat.nat_traversal =

#Configure the STUN server address.
account.2.nat.stun_server = 

#Configure the STUN server port, the default value is 3478.
account.2.nat.stun_port = 

#Enable or disable the NAT keep-alive; 0-Disabled, 1-Enabled (default);
account.2.nat.udp_update_enable = 

#Specify the keep-alive interval (in seconds), the default value is 30.
account.2.nat.udp_update_time = 

#Enable or disable the NAT Rport; 0-Disabled (default), 1-Enabled;
account.2.nat.rport = 

#Configure the session timer (in seconds), the default values of T1, T2, T3 are 0.5, 4, 5.
account.2.advanced.timer_t1 = 
account.2.advanced.timer_t2 = 
account.2.advanced.timer_t4 = 

account.2.codec.1.enable = 
account.2.codec.1.payload_type = 
account.2.codec.1.priority = 
account.2.codec.1.rtpmap = 

account.2.codec.2.enable = 
account.2.codec.2.payload_type = 
account.2.codec.2.priority =  
account.2.codec.2.rtpmap = 

account.2.codec.3.enable = 
account.2.codec.3.payload_type = 
account.2.codec.3.priority =
account.2.codec.3.rtpmap = 

account.2.codec.4.enable = 
account.2.codec.4.payload_type = 
account.2.codec.4.priority = 
account.2.codec.4.rtpmap = 

account.2.codec.5.enable = 
account.2.codec.5.payload_type = 
account.2.codec.5.priority = 
account.2.codec.5.rtpmap = 

account.2.codec.6.enable = 
account.2.codec.6.payload_type = 
account.2.codec.6.priority = 
account.2.codec.6.rtpmap = 

account.2.codec.7.enable = 
account.2.codec.7.payload_type = 
account.2.codec.7.priority = 
account.2.codec.7.rtpmap = 

account.2.codec.8.enable =  
account.2.codec.8.payload_type = 
account.2.codec.8.priority = 
account.2.codec.8.rtpmap = 

account.2.codec.9.enable = 
account.2.codec.9.payload_type = 
account.2.codec.9.priority = 
account.2.codec.9.rtpmap = 

#######################################################################################
##         	                   Call Forward                                          ##               
#######################################################################################
#Enable or disable the always forward, 0-Disabled(default), 1-Enabled;
account.2.always_fwd.enable = 

#Configure the target phonenumber that the phone will forward the call to;
account.2.always_fwd.target = 




#Enable or disable the busy forward, 0-Disabled(default), 1-Enabled;
account.2.busy_fwd.enable =         
account.2.busy_fwd.target = 



#Enable or disable the no answer forward, 0-Disabled(default), 1-Enabled; 
#Configure the waiting ring times before forwarding, ranges from 0 to 20 (by default);
account.2.timeout_fwd.enable = 
account.2.timeout_fwd.target =
account.2.timeout_fwd.timeout =  


 

#######################################################################################
##                          DND                                                      ##                                       
#######################################################################################



#Enable or disable the DND feautre for account2; 0-Disabled (default), 1-Enabled;
account.2.dnd.enable =  


#######################################################################################
##                           Register Advanced                                       ##       
#######################################################################################
account.2.sip_server_type = 
account.2.unregister_on_reboot = 
account.2.sip_trust_ctrl = 
account.2.proxy_require = 
account.2.srv_ttl_timer_enable = 

#######################################################################################
##                                   Network Conference                              ##                                       
#######################################################################################
account.2.conf_type = 
account.2.conf_uri = 

#######################################################################################
##                                   Account3 Settings                               ##                                       
#######################################################################################

#Enable or disable the account 1; 0-Disabled (default), 1-Enabled;
account.3.enable = %BWLINE-BINARY-3%

#Configure the label displayed on the LCD screen for account 1.
account.3.label = %BWEXTENSION-3%

#Configure the display name of account 1.
account.3.display_name = %BWCLID-3%

#Configure the username and password for register authentication.
account.3.auth_name = %BWAUTHUSER-3%
account.3.password = %BWAUTHPASSWORD-3%

#Configure the register user name.
account.3.user_name = %BWLINEPORT-3%



#Enable or disable to use the outbound proxy server; 0-Disabled (default), 1-Enabled; 
account.3.outbound_proxy_enable = 1

#Specify the IP address or domain name of the outbound proxy server.
account.3.outbound_host = %SBC_ADDRESS%

#Specify the server port, the default value is 5060.
account.3.outbound_port = %SBC_PORT%

#Configure the transport type; 0-UDP (default), 1-TCP, 2-TLS, 3-DNS SRV;
account.3.transport = %TRANSPORT_TYPE%

 
voice_mail.number.3 = %BWVOICE-PORTAL-NUMBER-3% 
account.3.anonymous_call_mode =
account.3.reject_anonymous_call_mode =

#Enable or disable the anonymous call feature; 0-Disabled (default), 1-Enabled;
account.3.anonymous_call = 

#Configure the on code and off code of the anonymous call feature.
account.3.send_anonymous_code =
account.3.anonymous_call_oncode = 
account.3.anonymous_call_offcode = 

#Enable or disable the reject anonymous call feature; 0-Disabled (default), 1-Enabled;
account.3.reject_anonymous_call = %REJECT_ANONYMOUS_CALL_BINARY%

#Configure the on code and off code of the reject anonymous call feature.
account.3.send_anonymous_rejection_code =
account.3.anonymous_reject_oncode = 
account.3.anonymous_reject_offcode = 

#Configure the SIP port for account 1, the default value is 5060. 
account.3.sip_listen_port = 

#Configure the register expiry time (in seconds), the default value is 3600.
account.3.expires = 

#Enable or disable the 100 reliable retransmission; 0-Disabled, 1-Enabled (default);
account.3.100rel_enable =


#Enable or disable the phone to subscribe the register status; 0-Disabled (default), 1-Enabled;
account.3.subscribe_register =

#Enable or disable the phone to subscribe the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.3.subscribe_mwi = 

#Configure MWI subscribe expiry time (in seconds). It ranges from 0 to 84600, the default value is 3600.
account.3.subscribe_mwi_expires = 

#Configure the type of SIP header to carry the caller ID; 0-FROM (default), 1-PAI;
account.3.cid_source = 
 
#Enable or disable the session timer; 0-Disabled (default), 1-Enabled;  
account.3.session_timer.enable =       

#Configure the refresh session timer interval (in seconds). It ranges from 1 to 9999.
account.3.session_timer.expires =           

#Configure the session timer refresher; 0-Uac (default), 1-Uas;
account.3.session_timer.refresher = 

#Enable or disable the "user=phone"; 0-Disabled (default), 1-Enabled;
account.3.enable_user_equal_phone = 

#Configure the way of encrypting the message; 0-Disabled (default), 1-Forced, 2-Negotiated;
account.3.srtp_encryption = 

#Configure the RTP packet time. The valid values are 0 (Disabled), 10, 20 (default), 30, 40, 50, 60.
account.3.ptime =  

#Enable or disable the phone to subscribe to the voicemail through the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.3.subscribe_mwi_to_vm = 

#Enable or disable the phone to send the MAC address in the Register message; 0-Disabled (default), 1-Enabled;    
account.3.register_mac =

#Enable or disable the phone to send the line number in the Register message; 0-Disabled, 1-Enabled (default);   
account.3.register_line = 

#Configure the interval (in seconds) the phone retries to register when account 1 fails to register. It ranges from 0 to 1800, the default value is 30.
account.3.reg_fail_retry_interval = 

#Configure the DTMF type; 0-INBAND, 1-RFC2833 (default), 2-SIP INFO, 3-AUTO+SIP INFO;
account.3.dtmf.type =

#Configure the RFC2833 payload. It ranges from 96 to 225, the default value is 101.
account.3.dtmf.dtmf_payload = 

#Configure the DTMF info type when using the SIP INFO; 0-Disabled, 1-DTMF-Relay (default), 2-DTMF, 3-Telephone-Event;
account.3.dtmf.info_type = 

account.3.auto_dial_num = 
account.3.auto_dial_enable = 

account.3.cid_source_privacy = 
account.3.cid_source_ppi = 
account.3.cp_source = 

voice_mail.number.3 = 
account.3.shared_line = 
#######################################################################################
##                          Failback                                                 ##       
#######################################################################################
account.3.naptr_build = 
account.3.fallback.redundancy_type = 
account.3.fallback.timeout = 
account.3.sip_server.1.address =
account.3.sip_server.1.port = 
account.3.sip_server.1.expires = 
account.3.sip_server.1.retry_counts = 
account.3.sip_server.1.failback_mode = 
account.3.sip_server.1.failback_timeout = 
account.3.sip_server.1.register_on_enable = 

account.3.sip_server.2.address =
account.3.sip_server.2.port = 
account.3.sip_server.2.expires = 
account.3.sip_server.2.retry_counts = 
account.3.sip_server.2.failback_mode = 
account.3.sip_server.2.failback_timeout = 
account.3.sip_server.2.register_on_enable = 

account.3.dns_cache_type = 
account.3.dns_cache_a.1.name =
account.3.dns_cache_a.1.ip =
account.3.dns_cache_a.1.ttl = 
account.3.dns_cache_srv.1.name =
account.3.dns_cache_srv.1.port = 
account.3.dns_cache_srv.1.priority = 
account.3.dns_cache_srv.1.target =
account.3.dns_cache_srv.1.weight = 
account.3.dns_cache_srv.1.ttl = 
account.3.dns_cache_naptr.1.name =
account.3.dns_cache_naptr.1.flags =
account.3.dns_cache_naptr.1.order = 
account.3.dns_cache_naptr.1.preference = 
account.3.dns_cache_naptr.1.replace =
account.3.dns_cache_naptr.1.service =
account.3.dns_cache_naptr.1.ttl = 


account.3.dns_cache_a.2.name =
account.3.dns_cache_a.2.ip =
account.3.dns_cache_a.2.ttl = 
account.3.dns_cache_srv.2.name =
account.3.dns_cache_srv.2.port = 
account.3.dns_cache_srv.2.priority = 
account.3.dns_cache_srv.2.target =
account.3.dns_cache_srv.2.weight = 
account.3.dns_cache_srv.2.ttl = 
account.3.dns_cache_naptr.2.name =
account.3.dns_cache_naptr.2.flags =
account.3.dns_cache_naptr.2.order = 
account.3.dns_cache_naptr.2.preference = 
account.3.dns_cache_naptr.2.replace =
account.3.dns_cache_naptr.2.service =
account.3.dns_cache_naptr.2.ttl = 

account.3.static_cache_pri = 






#######################################################################################
##                                   NAT Settings                                    ##
#######################################################################################

#Enable or disable the NAT traversal; 0-Disabled (default), 1-STUN;
account.3.nat.nat_traversal =

#Configure the STUN server address.
account.3.nat.stun_server = 

#Configure the STUN server port, the default value is 3478.
account.3.nat.stun_port = 

#Enable or disable the NAT keep-alive; 0-Disabled, 1-Enabled (default);
account.3.nat.udp_update_enable = 

#Specify the keep-alive interval (in seconds), the default value is 30.
account.3.nat.udp_update_time = 

#Enable or disable the NAT Rport; 0-Disabled (default), 1-Enabled;
account.3.nat.rport = 

#Configure the session timer (in seconds), the default values of T1, T2, T3 are 0.5, 4, 5.
account.3.advanced.timer_t1 = 
account.3.advanced.timer_t2 = 
account.3.advanced.timer_t4 = 

account.3.codec.1.enable = 
account.3.codec.1.payload_type = 
account.3.codec.1.priority = 
account.3.codec.1.rtpmap = 

account.3.codec.2.enable = 
account.3.codec.2.payload_type = 
account.3.codec.2.priority =  
account.3.codec.2.rtpmap = 

account.3.codec.3.enable = 
account.3.codec.3.payload_type = 
account.3.codec.3.priority =
account.3.codec.3.rtpmap = 

account.3.codec.4.enable = 
account.3.codec.4.payload_type = 
account.3.codec.4.priority = 
account.3.codec.4.rtpmap = 

account.3.codec.5.enable = 
account.3.codec.5.payload_type = 
account.3.codec.5.priority = 
account.3.codec.5.rtpmap = 

account.3.codec.6.enable = 
account.3.codec.6.payload_type = 
account.3.codec.6.priority = 
account.3.codec.6.rtpmap = 

account.3.codec.7.enable = 
account.3.codec.7.payload_type = 
account.3.codec.7.priority = 
account.3.codec.7.rtpmap = 

account.3.codec.8.enable =  
account.3.codec.8.payload_type = 
account.3.codec.8.priority = 
account.3.codec.8.rtpmap = 

account.3.codec.9.enable = 
account.3.codec.9.payload_type = 
account.3.codec.9.priority = 
account.3.codec.9.rtpmap = 

#######################################################################################
##         	                   Call Forward                                          ##               
#######################################################################################
#Enable or disable the always forward, 0-Disabled(default), 1-Enabled;
account.3.always_fwd.enable = 

#Configure the target phonenumber that the phone will forward the call to;
account.3.always_fwd.target = 




#Enable or disable the busy forward, 0-Disabled(default), 1-Enabled;
account.3.busy_fwd.enable =         
account.3.busy_fwd.target = 



#Enable or disable the no answer forward, 0-Disabled(default), 1-Enabled; 
#Configure the waiting ring times before forwarding, ranges from 0 to 20 (by default);
account.3.timeout_fwd.enable = 
account.3.timeout_fwd.target =
account.3.timeout_fwd.timeout =  


  

#######################################################################################
##                          DND                                                      ##                                       
#######################################################################################



#Enable or disable the DND feautre for account3; 0-Disabled (default), 1-Enabled;
account.3.dnd.enable =  



#######################################################################################
##                           Register Advanced                                       ##       
#######################################################################################
account.3.sip_server_type = 
account.3.unregister_on_reboot = 
account.3.sip_trust_ctrl = 
account.3.proxy_require = 
account.3.srv_ttl_timer_enable = 

#######################################################################################
##                                   Network Conference                              ##                                       
#######################################################################################
account.3.conf_type = 
account.3.conf_uri = 

#######################################################################################
##                                   Account4 Settings                               ##                                       
#######################################################################################

#Enable or disable the account 1; 0-Disabled (default), 1-Enabled;
account.4.enable = %BWLINE-BINARY-4%

#Configure the label displayed on the LCD screen for account 1.
account.4.label = %BWEXTENSION-4%

#Configure the display name of account 1.
account.4.display_name = %BWCLID-4%

#Configure the username and password for register authentication.
account.4.auth_name = %BWAUTHUSER-4%
account.4.password = %BWAUTHPASSWORD-4%

#Configure the register user name.
account.4.user_name = %BWLINEPORT-4%



#Enable or disable to use the outbound proxy server; 0-Disabled (default), 1-Enabled; 
account.4.outbound_proxy_enable = 1

#Specify the IP address or domain name of the outbound proxy server.
account.4.outbound_host = %SBC_ADDRESS%

#Specify the server port, the default value is 5060.
account.4.outbound_port = %SBC_PORT%

#Configure the transport type; 0-UDP (default), 1-TCP, 2-TLS, 3-DNS SRV;
account.4.transport = %TRANSPORT_TYPE%

voice_mail.number.4 = %BWVOICE-PORTAL-NUMBER-4% 
account.4.anonymous_call_mode =
account.4.reject_anonymous_call_mode =

#Enable or disable the anonymous call feature; 0-Disabled (default), 1-Enabled;
account.4.anonymous_call = 

#Configure the on code and off code of the anonymous call feature.
account.4.send_anonymous_code =
account.4.anonymous_call_oncode = 
account.4.anonymous_call_offcode = 

#Enable or disable the reject anonymous call feature; 0-Disabled (default), 1-Enabled;
account.4.reject_anonymous_call = %REJECT_ANONYMOUS_CALL_BINARY%

#Configure the on code and off code of the reject anonymous call feature.
account.4.send_anonymous_rejection_code =
account.4.anonymous_reject_oncode = 
account.4.anonymous_reject_offcode = 

#Configure the SIP port for account 1, the default value is 5060. 
account.4.sip_listen_port = 

#Configure the register expiry time (in seconds), the default value is 3600.
account.4.expires = 

#Enable or disable the 100 reliable retransmission; 0-Disabled, 1-Enabled (default);
account.4.100rel_enable =


#Enable or disable the phone to subscribe the register status; 0-Disabled (default), 1-Enabled;
account.4.subscribe_register =

#Enable or disable the phone to subscribe the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.4.subscribe_mwi = 

#Configure MWI subscribe expiry time (in seconds). It ranges from 0 to 84600, the default value is 3600.
account.4.subscribe_mwi_expires = 

#Configure the type of SIP header to carry the caller ID; 0-FROM (default), 1-PAI;
account.4.cid_source = 
 
#Enable or disable the session timer; 0-Disabled (default), 1-Enabled;  
account.4.session_timer.enable =       

#Configure the refresh session timer interval (in seconds). It ranges from 1 to 9999.
account.4.session_timer.expires =           

#Configure the session timer refresher; 0-Uac (default), 1-Uas;
account.4.session_timer.refresher = 

#Enable or disable the "user=phone"; 0-Disabled (default), 1-Enabled;
account.4.enable_user_equal_phone = 

#Configure the way of encrypting the message; 0-Disabled (default), 1-Forced, 2-Negotiated;
account.4.srtp_encryption = 

#Configure the RTP packet time. The valid values are 0 (Disabled), 10, 20 (default), 30, 40, 50, 60.
account.4.ptime =  

#Enable or disable the phone to subscribe to the voicemail through the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.4.subscribe_mwi_to_vm = 

#Enable or disable the phone to send the MAC address in the Register message; 0-Disabled (default), 1-Enabled;    
account.4.register_mac =

#Enable or disable the phone to send the line number in the Register message; 0-Disabled, 1-Enabled (default);   
account.4.register_line = 

#Configure the interval (in seconds) the phone retries to register when account 1 fails to register. It ranges from 0 to 1800, the default value is 30.
account.4.reg_fail_retry_interval = 

#Configure the DTMF type; 0-INBAND, 1-RFC2833 (default), 2-SIP INFO, 3-AUTO+SIP INFO;
account.4.dtmf.type =

#Configure the RFC2833 payload. It ranges from 96 to 225, the default value is 101.
account.4.dtmf.dtmf_payload = 

#Configure the DTMF info type when using the SIP INFO; 0-Disabled, 1-DTMF-Relay (default), 2-DTMF, 3-Telephone-Event;
account.4.dtmf.info_type = 

account.4.auto_dial_num = 
account.4.auto_dial_enable = 

account.4.cid_source_privacy = 
account.4.cid_source_ppi = 
account.4.cp_source = 

voice_mail.number.4 = 

account.4.shared_line = 
#######################################################################################
##                          Failback                                                 ##       
#######################################################################################
account.4.naptr_build = 
account.4.fallback.redundancy_type = 
account.4.fallback.timeout = 
account.4.sip_server.1.address =
account.4.sip_server.1.port = 
account.4.sip_server.1.expires = 
account.4.sip_server.1.retry_counts = 
account.4.sip_server.1.failback_mode = 
account.4.sip_server.1.failback_timeout = 
account.4.sip_server.1.register_on_enable = 

account.4.sip_server.2.address =
account.4.sip_server.2.port = 
account.4.sip_server.2.expires = 
account.4.sip_server.2.retry_counts = 
account.4.sip_server.2.failback_mode = 
account.4.sip_server.2.failback_timeout = 
account.4.sip_server.2.register_on_enable = 

account.4.dns_cache_type = 
account.4.dns_cache_a.1.name =
account.4.dns_cache_a.1.ip =
account.4.dns_cache_a.1.ttl = 
account.4.dns_cache_srv.1.name =
account.4.dns_cache_srv.1.port = 
account.4.dns_cache_srv.1.priority = 
account.4.dns_cache_srv.1.target =
account.4.dns_cache_srv.1.weight = 
account.4.dns_cache_srv.1.ttl = 
account.4.dns_cache_naptr.1.name =
account.4.dns_cache_naptr.1.flags =
account.4.dns_cache_naptr.1.order = 
account.4.dns_cache_naptr.1.preference = 
account.4.dns_cache_naptr.1.replace =
account.4.dns_cache_naptr.1.service =
account.4.dns_cache_naptr.1.ttl = 


account.4.dns_cache_a.2.name =
account.4.dns_cache_a.2.ip =
account.4.dns_cache_a.2.ttl = 
account.4.dns_cache_srv.2.name =
account.4.dns_cache_srv.2.port = 
account.4.dns_cache_srv.2.priority = 
account.4.dns_cache_srv.2.target =
account.4.dns_cache_srv.2.weight = 
account.4.dns_cache_srv.2.ttl = 
account.4.dns_cache_naptr.2.name =
account.4.dns_cache_naptr.2.flags =
account.4.dns_cache_naptr.2.order = 
account.4.dns_cache_naptr.2.preference = 
account.4.dns_cache_naptr.2.replace =
account.4.dns_cache_naptr.2.service =
account.4.dns_cache_naptr.2.ttl = 

account.4.static_cache_pri = 



#######################################################################################
##                                   NAT Settings                                    ##
#######################################################################################

#Enable or disable the NAT traversal; 0-Disabled (default), 1-STUN;
account.4.nat.nat_traversal =

#Configure the STUN server address.
account.4.nat.stun_server = 

#Configure the STUN server port, the default value is 3478.
account.4.nat.stun_port = 

#Enable or disable the NAT keep-alive; 0-Disabled, 1-Enabled (default);
account.4.nat.udp_update_enable = 

#Specify the keep-alive interval (in seconds), the default value is 30.
account.4.nat.udp_update_time = 

#Enable or disable the NAT Rport; 0-Disabled (default), 1-Enabled;
account.4.nat.rport = 

#Configure the session timer (in seconds), the default values of T1, T2, T3 are 0.5, 4, 5.
account.4.advanced.timer_t1 = 
account.4.advanced.timer_t2 = 
account.4.advanced.timer_t4 = 


account.4.codec.1.enable = 
account.4.codec.1.payload_type = 
account.4.codec.1.priority = 
account.4.codec.1.rtpmap = 

account.4.codec.2.enable = 
account.4.codec.2.payload_type = 
account.4.codec.2.priority =  
account.4.codec.2.rtpmap = 

account.4.codec.3.enable = 
account.4.codec.3.payload_type = 
account.4.codec.3.priority =
account.4.codec.3.rtpmap = 

account.4.codec.4.enable = 
account.4.codec.4.payload_type = 
account.4.codec.4.priority = 
account.4.codec.4.rtpmap = 

account.4.codec.5.enable = 
account.4.codec.5.payload_type = 
account.4.codec.5.priority = 
account.4.codec.5.rtpmap = 

account.4.codec.6.enable = 
account.4.codec.6.payload_type = 
account.4.codec.6.priority = 
account.4.codec.6.rtpmap = 

account.4.codec.7.enable = 
account.4.codec.7.payload_type = 
account.4.codec.7.priority = 
account.4.codec.7.rtpmap = 

account.4.codec.8.enable =  
account.4.codec.8.payload_type = 
account.4.codec.8.priority = 
account.4.codec.8.rtpmap = 

account.4.codec.9.enable = 
account.4.codec.9.payload_type = 
account.4.codec.9.priority = 
account.4.codec.9.rtpmap = 

#######################################################################################
##         	                   Call Forward                                          ##               
#######################################################################################
#Enable or disable the always forward, 0-Disabled(default), 1-Enabled;
account.4.always_fwd.enable = 

#Configure the target phonenumber that the phone will forward the call to;
account.4.always_fwd.target = 



#Enable or disable the busy forward, 0-Disabled(default), 1-Enabled;
account.4.busy_fwd.enable =         
account.4.busy_fwd.target = 



#Enable or disable the no answer forward, 0-Disabled(default), 1-Enabled; 
#Configure the waiting ring times before forwarding, ranges from 0 to 20 (by default);
account.4.timeout_fwd.enable = 
account.4.timeout_fwd.target =
account.4.timeout_fwd.timeout =  


   

#######################################################################################
##                          DND                                                      ##                                       
#######################################################################################



#Enable or disable the DND feautre for account4; 0-Disabled (default), 1-Enabled;
account.4.dnd.enable =  



#######################################################################################
##                           Register Advanced                                       ##       
#######################################################################################
account.4.sip_server_type = 
account.4.unregister_on_reboot = 
account.4.sip_trust_ctrl = 
account.4.proxy_require = 
account.4.srv_ttl_timer_enable = 

#######################################################################################
##                                   Network Conference                              ##                                       
#######################################################################################
account.4.conf_type = 
account.4.conf_uri = 

#######################################################################################
##                                   Account5 Settings                               ##                                       
#######################################################################################

#Enable or disable the account 1; 0-Disabled (default), 1-Enabled;
account.5.enable = %BWLINE-BINARY-5%

#Configure the label displayed on the LCD screen for account 1.
account.5.label = %BWEXTENSION-5%

#Configure the display name of account 1.
account.5.display_name = %BWCLID-5%

#Configure the username and password for register authentication.
account.5.auth_name = %BWAUTHUSER-5%
account.5.password = %BWAUTHPASSWORD-5%

#Configure the register user name.
account.5.user_name = %BWLINEPORT-5%



#Enable or disable to use the outbound proxy server; 0-Disabled (default), 1-Enabled; 
account.5.outbound_proxy_enable = 1

#Specify the IP address or domain name of the outbound proxy server.
account.5.outbound_host = %SBC_ADDRESS%

#Specify the server port, the default value is 5060.
account.5.outbound_port = %SBC_PORT%

#Configure the transport type; 0-UDP (default), 1-TCP, 2-TLS, 3-DNS SRV;
account.5.transport = %TRANSPORT_TYPE%

voice_mail.number.5 = %BWVOICE-PORTAL-NUMBER-5% 
account.5.anonymous_call_mode =
account.5.reject_anonymous_call_mode =

#Enable or disable the anonymous call feature; 0-Disabled (default), 1-Enabled;
account.5.anonymous_call = 

#Configure the on code and off code of the anonymous call feature.
account.5.send_anonymous_code =
account.5.anonymous_call_oncode = 
account.5.anonymous_call_offcode = 

#Enable or disable the reject anonymous call feature; 0-Disabled (default), 1-Enabled;
account.5.reject_anonymous_call = %REJECT_ANONYMOUS_CALL_BINARY%

#Configure the on code and off code of the reject anonymous call feature.
account.5.send_anonymous_rejection_code =
account.5.anonymous_reject_oncode = 
account.5.anonymous_reject_offcode = 

#Configure the SIP port for account 1, the default value is 5060. 
account.5.sip_listen_port = 

#Configure the register expiry time (in seconds), the default value is 3600.
account.5.expires = 

#Enable or disable the 100 reliable retransmission; 0-Disabled, 1-Enabled (default);
account.5.100rel_enable =


#Enable or disable the phone to subscribe the register status; 0-Disabled (default), 1-Enabled;
account.5.subscribe_register =

#Enable or disable the phone to subscribe the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.5.subscribe_mwi = 

#Configure MWI subscribe expiry time (in seconds). It ranges from 0 to 84600, the default value is 3600.
account.5.subscribe_mwi_expires = 

#Configure the type of SIP header to carry the caller ID; 0-FROM (default), 1-PAI;
account.5.cid_source = 
 
#Enable or disable the session timer; 0-Disabled (default), 1-Enabled;  
account.5.session_timer.enable =       

#Configure the refresh session timer interval (in seconds). It ranges from 1 to 9999.
account.5.session_timer.expires =           

#Configure the session timer refresher; 0-Uac (default), 1-Uas;
account.5.session_timer.refresher = 

#Enable or disable the "user=phone"; 0-Disabled (default), 1-Enabled;
account.5.enable_user_equal_phone = 

#Configure the way of encrypting the message; 0-Disabled (default), 1-Forced, 2-Negotiated;
account.5.srtp_encryption = 

#Configure the RTP packet time. The valid values are 0 (Disabled), 10, 20 (default), 30, 40, 50, 60.
account.5.ptime =  

#Enable or disable the phone to subscribe to the voicemail through the message waiting indicator; 0-Disabled (default), 1-Enabled;
account.5.subscribe_mwi_to_vm = 

#Enable or disable the phone to send the MAC address in the Register message; 0-Disabled (default), 1-Enabled;    
account.5.register_mac =

#Enable or disable the phone to send the line number in the Register message; 0-Disabled, 1-Enabled (default);   
account.5.register_line = 

#Configure the interval (in seconds) the phone retries to register when account 1 fails to register. It ranges from 0 to 1800, the default value is 30.
account.5.reg_fail_retry_interval = 

#Configure the DTMF type; 0-INBAND, 1-RFC2833 (default), 2-SIP INFO, 3-AUTO+SIP INFO;
account.5.dtmf.type =

#Configure the RFC2833 payload. It ranges from 96 to 225, the default value is 101.
account.5.dtmf.dtmf_payload = 

#Configure the DTMF info type when using the SIP INFO; 0-Disabled, 1-DTMF-Relay (default), 2-DTMF, 3-Telephone-Event;
account.5.dtmf.info_type = 

account.5.auto_dial_num = 
account.5.auto_dial_enable = 

account.5.cid_source_privacy = 
account.5.cid_source_ppi = 
account.5.cp_source = 

voice_mail.number.5 = 

account.5.shared_line = 
#######################################################################################
##                          Failback                                                 ##       
#######################################################################################
account.5.naptr_build = 
account.5.fallback.redundancy_type = 
account.5.fallback.timeout = 
account.5.sip_server.1.address =
account.5.sip_server.1.port = 
account.5.sip_server.1.expires = 
account.5.sip_server.1.retry_counts = 
account.5.sip_server.1.failback_mode = 
account.5.sip_server.1.failback_timeout = 
account.5.sip_server.1.register_on_enable = 

account.5.sip_server.2.address =
account.5.sip_server.2.port = 
account.5.sip_server.2.expires = 
account.5.sip_server.2.retry_counts = 
account.5.sip_server.2.failback_mode = 
account.5.sip_server.2.failback_timeout = 
account.5.sip_server.2.register_on_enable = 

account.5.dns_cache_type = 
account.5.dns_cache_a.1.name =
account.5.dns_cache_a.1.ip =
account.5.dns_cache_a.1.ttl = 
account.5.dns_cache_srv.1.name =
account.5.dns_cache_srv.1.port = 
account.5.dns_cache_srv.1.priority = 
account.5.dns_cache_srv.1.target =
account.5.dns_cache_srv.1.weight = 
account.5.dns_cache_srv.1.ttl = 
account.5.dns_cache_naptr.1.name =
account.5.dns_cache_naptr.1.flags =
account.5.dns_cache_naptr.1.order = 
account.5.dns_cache_naptr.1.preference = 
account.5.dns_cache_naptr.1.replace =
account.5.dns_cache_naptr.1.service =
account.5.dns_cache_naptr.1.ttl = 


account.5.dns_cache_a.2.name =
account.5.dns_cache_a.2.ip =
account.5.dns_cache_a.2.ttl = 
account.5.dns_cache_srv.2.name =
account.5.dns_cache_srv.2.port = 
account.5.dns_cache_srv.2.priority = 
account.5.dns_cache_srv.2.target =
account.5.dns_cache_srv.2.weight = 
account.5.dns_cache_srv.2.ttl = 
account.5.dns_cache_naptr.2.name =
account.5.dns_cache_naptr.2.flags =
account.5.dns_cache_naptr.2.order = 
account.5.dns_cache_naptr.2.preference = 
account.5.dns_cache_naptr.2.replace =
account.5.dns_cache_naptr.2.service =
account.5.dns_cache_naptr.2.ttl = 

account.5.static_cache_pri = 






#######################################################################################
##                                   NAT Settings                                    ##
#######################################################################################

#Enable or disable the NAT traversal; 0-Disabled (default), 1-STUN;
account.5.nat.nat_traversal =

#Configure the STUN server address.
account.5.nat.stun_server = 

#Configure the STUN server port, the default value is 3478.
account.5.nat.stun_port = 

#Enable or disable the NAT keep-alive; 0-Disabled, 1-Enabled (default);
account.5.nat.udp_update_enable = 

#Specify the keep-alive interval (in seconds), the default value is 30.
account.5.nat.udp_update_time = 

#Enable or disable the NAT Rport; 0-Disabled (default), 1-Enabled;
account.5.nat.rport = 

#Configure the session timer (in seconds), the default values of T1, T2, T3 are 0.5, 4, 5.
account.5.advanced.timer_t1 = 
account.5.advanced.timer_t2 = 
account.5.advanced.timer_t4 = 

account.5.codec.1.enable = 
account.5.codec.1.payload_type = 
account.5.codec.1.priority = 
account.5.codec.1.rtpmap = 

account.5.codec.2.enable = 
account.5.codec.2.payload_type = 
account.5.codec.2.priority =  
account.5.codec.2.rtpmap = 

account.5.codec.3.enable = 
account.5.codec.3.payload_type = 
account.5.codec.3.priority =
account.5.codec.3.rtpmap = 

account.5.codec.4.enable = 
account.5.codec.4.payload_type = 
account.5.codec.4.priority = 
account.5.codec.4.rtpmap = 

account.5.codec.5.enable = 
account.5.codec.5.payload_type = 
account.5.codec.5.priority = 
account.5.codec.5.rtpmap = 

account.5.codec.6.enable = 
account.5.codec.6.payload_type = 
account.5.codec.6.priority = 
account.5.codec.6.rtpmap = 

account.5.codec.7.enable = 
account.5.codec.7.payload_type = 
account.5.codec.7.priority = 
account.5.codec.7.rtpmap = 

account.5.codec.8.enable =  
account.5.codec.8.payload_type = 
account.5.codec.8.priority = 
account.5.codec.8.rtpmap = 

account.5.codec.9.enable = 
account.5.codec.9.payload_type = 
account.5.codec.9.priority = 
account.5.codec.9.rtpmap = 

#######################################################################################
##         	                   Call Forward                                          ##               
#######################################################################################
#Enable or disable the always forward, 0-Disabled(default), 1-Enabled;
account.5.always_fwd.enable = 

#Configure the target phonenumber that the phone will forward the call to;
account.5.always_fwd.target = 



#Enable or disable the busy forward, 0-Disabled(default), 1-Enabled;
account.5.busy_fwd.enable =         
account.5.busy_fwd.target = 



#Enable or disable the no answer forward, 0-Disabled(default), 1-Enabled; 
#Configure the waiting ring times before forwarding, ranges from 0 to 20 (by default);
account.5.timeout_fwd.enable = 
account.5.timeout_fwd.target =
account.5.timeout_fwd.timeout =  


   

#######################################################################################
##                          DND                                                      ##                                       
#######################################################################################



#Enable or disable the DND feautre for account5; 0-Disabled (default), 1-Enabled;
account.5.dnd.enable = 



#######################################################################################
##                           Register Advanced                                       ##       
#######################################################################################
account.5.sip_server_type = 
account.5.unregister_on_reboot = 
account.5.sip_trust_ctrl = 
account.5.proxy_require = 
account.5.srv_ttl_timer_enable = 

#######################################################################################
##                                   Network Conference                              ##                                       
#######################################################################################
account.5.conf_type = 
account.5.conf_uri = 


#######################################################################################
##                                   Network                                         ## 
#######################################################################################

#Configure the WAN port type; 0-DHCP(default), 1-PPPoE, 2-Static IP Address;
#Require reboot;
network.internet_port.type = 

# 0-Disable(default),1-Enable;
network.static_dns_enable =       

#Configure the static IP address, submask, gateway and DNS server.
#Require reboot;
network.internet_port.ip = 
network.internet_port.mask = 
network.internet_port.gateway = 
network.primary_dns= %DNS_SERVER_1%
network.secondary_dns = %DNS_SERVER_2%                               


#######################################################################################
##                                   Time Settings                                   ##
#######################################################################################

#Configure the time zone and time zone name. The time zone ranges from -11 to +12, the default value is +8. 
#The default time zone name is China(Beijing).   
#local_time.time_zone = +8
#local_time.time_zone_name = China(Beijing) 
local_time.time_zone =
local_time.time_zone_name = 

#Configure the domain name or the IP address of the NTP server. The default value is cn.pool.ntp.org.
local_time.ntp_server1 = %SNTP_SERVER_1%
local_time.ntp_server2 = %SNTP_SERVER_2%

#Configure the update interval (in seconds) when using the NTP server. The default value is 1000.
local_time.interval = 

#Configure the daylight saving time feature; 0-Disabled, 1-Enabled, 2-Automatic (default); 
local_time.summer_time = 

#Configure the DST type when the DST feature is enabled; 0-By Date (default), 1-By Week;
local_time.dst_time_type = 

#Configure the start time of DST. The default value is 1/1/0.
#If the DST type is configured as By Date, the value format is Month/Day/Hour. For example, the value 5/20/10 means the start time is at 10:00 on May 20.  
#If the DST type is configured as By Week, the value format is Month/Day of Week/Day of Week Last in Month/Hour of Day. 
#For example, the value 1/4/2/5 means the start time is at 5 o'clock on Tuesday of the 4th week in January.
local_time.start_time = 

#Configure the end time of DST. The default value is 12/31/23. The value format is the same to the start time.
local_time.end_time = 

#Configure the offset time (in minutes). It ranges from -300 to 300, the default value is 60.
local_time.offset_time = 

#Enable or disable the DHCP time, 0-Disabled (default), 1-Enabled;
local_time.dhcp_time = 

auto_dst.url = http://%BWDEVICEACCESSFQDN%:%BWDEVICEACCESSPORT%/%BWDMSCONTEXT%/%BWDEVICEACCESSURI%Autodst.xml

0-Disabled (default), 1-Enabled;
local_time.manual_time_enable = 

local_time.manual_ntp_srv_prior =

#######################################################################################
##                                   Tone                                            ##                                            
#######################################################################################
voice.tone.country = %COUNTRY%
voice.tone.dial = 
voice.tone.ring = 
voice.tone.busy = 
voice.tone.callwaiting =  

#######################################################################################
##                                   Language Settings                               ##       
#######################################################################################

#Specify the web language, the valid values are: English, Chinese_S, German, Italian and Turkish;
lang.wui = %LANGUAGEWEB%


#######################################################################################
##                                   Auto Provisioning                               ##      
#######################################################################################

#Configure the username and password for downloading.
auto_provision.server.username = %BWDEVICEUSERNAME%
auto_provision.server.password = %DEVICE_ACCESS_PWD%


